FRONT DOOR WILL NOT STAY OPEN ON A SLIGHT INCLINE-NEW SPRING. Buick Coachbuilder 1991

For 1990-2009 cars

# FRONT DOOR WILL NOT STAY OPEN ON A SLIGHT INCLINE-NEW SPRING

#### SUBJECT: FRONT DOORS WON'T HOLD OPEN ON SLIGHT INCLINE/FRONT DOORS HARD TO OPEN (REPLACE DOOR HOLD OPEN SPRING)

#### MODELS AFFECTED: 1991 ROADMASTER ESTATE WAGON

CONDITION: 1. Front Doors Won't Hold Open on Slight Incline 2. Front Doors Hard To Open

CAUSE: Door hold open spring is too weak or too strong.

CORRECTION: Replace door hold open spring with P/N 20361482 prior to the VIN MW400236.

#### Note: Replace both RH and LH Front Door Hold Open Springs at time of repair.

Parts are currently available from GMSPO.

Spring Removal Tool: A loaner tool program has been set up through Kent- Moore. Just call 1-800-345-2233 and ask for J-39079-LNR.

Due to the limited number of tools available, please schedule vehicles in a timely manner and return loan tool as soon as possible using the return label.

#### WARRANTY INFORMATION:

Labor Operation Number: RH B4050 LH B4051

Labor Time: .2 Hr. Per Side Material Allowance: GA

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.