WIND NOISE, ROOF LUGGAGE RACK/ CARRIERS REPOSITION FRT. RAIL. Buick Coachbuilder 1991

For 1990-2009 cars

# WIND NOISE, ROOF LUGGAGE RACK/ CARRIERS REPOSITION FRT. RAIL

#### SUBJECT: WINDNOISE, ROOF LUGGAGE CARRIERS (REPOSITION FRONT RAIL)

#### VEHICLES AFFECTED: 1991 CAPRICE WAGON

#### Condition:

---------- Some customers may comment about windnoise in the roof area on 1991 Caprice wagons when traveling at highway speeds.

#### Cause:

------- This condition may be due to wind buffeting on the front cross rail of the roof luggage carrier.

#### Correction:

----------- To reduce the potential of this condition, please inform the owner to position the front cross rail fully rearward when not in use as shown in the illustration.

#### Note: New cross rails will be available in the future to correct this condition.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.