FRONT DOOR LOCK ROD RATTLE (INSTALL NEW LOCK ROD CLIP). Buick Coachbuilder 1992

For 1990-2009 cars

# FRONT DOOR LOCK ROD RATTLE (INSTALL NEW LOCK ROD CLIP)

#### SUBJECT: FRONT DOOR LOCK ROD RATTLES (INSTALL NEW LOCK ROD CLIP)

#### VEHICLES AFFECTED: 1991-92 "B" - CARS CHEVROLET CAPRICE SEDAN/WAGON OLDSMOBILE CUSTOM CRUISER WAGON BUICK ROADMASTER SEDAN/WAGON

#### CONDITION:

---------- Front door lock rod rattles.

#### CORRECTION:

----------- Using kit P/N 10222731, install new style lock rod anti-rattle clip. Each kit contains one clip.

1. Remove the door trim pad and water deflector.

2. While holding the clip with the notched end away from you, (See View A) insert the notched end into the lock module first (See View B). Then insert the other end and rotate 90 degrees, making sure that the reinforced area of the clip faces downward (See View C).

#### Notice: Failure to orientate the lock rod clip properly may cause the lock rods to operate improperly.

3. Check for proper operation of the lock rods and reinstall the water deflector and trim pad.

For vehicles repaired under warranty use:

Labor Operation: B4360 - Right Hand B4361 - Left Hand Labor Time: 0.5 hour - Per Door

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.