NOISY DOOR TRIM PADS (INSTALL SCREWS). Buick Coachbuilder 1994

For 1990-2009 cars

# NOISY DOOR TRIM PADS (INSTALL SCREWS)

#### SUBJECT: NOISY DOOR TRIM PADS (INSTALL SCREWS)

#### MODELS: 1994 BUICK ROADMASTER

#### CONDITION:

SOME OWNERS MAY COMMENT ON NOISY DOOR TRIM PADS.

#### CAUSE:

ARMREST PAD IS LOOSE IN DOOR TRIM.

#### CORRECTION:

ADD SCREWS TO SECURE ARMREST.

1. REMOVE DOOR TRIM AND PLACE BACK SIDE UP ON A CLEAN WORK SURFACE.

2. PULL SOUND DEADENING MATERIAL AWAY FROM TRIM PAD ENOUGH TO EXPOSE ARMREST AREA.

3. INSTALL THREE (3) SCREWS, P/N 15603694, THROUGH HOLES ALREADY IN TRIM PANEL INTO BOSSES IN THE ARMREST. SEE FIGURE 1, ITEM 1.

4. REINSTALL TRIM TO DOOR INNER PANEL.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C3348 (RIGHT FRONT DOOR) C3358 (LEFT FRONT DOOR) C3540 (RIGHT REAR DOOR) C3541 (LEFT REAR DOOR)

USE PUBLISHED LABOR OPERATION TIME PLUS .1 TO INSTALL SCREWS.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.