REAR SUSPENSION SPRING CLUNK INSTALL LWR. SPRING INSULATOR. Buick Coachbuilder 1991

For 1990-2009 cars

# REAR SUSPENSION SPRING CLUNK INSTALL LWR. SPRING INSULATOR

#### SUBJECT: REAR SUSPENSION SPRING CLUNK (INSTALL SPRING LOWER INSULATORS)

#### MODELS AFFECTED: 1991 ROADMASTER ESTATE WAGONS

#### CONDITION:

----------- Some 1991 Roadmaster Estate Wagons assembled prior to VIN breakpoint MW406956 may exhibit a clunking type noise from the rear of the vehicle when being operated over irregular road surfaces.

#### CAUSE:

------- Rear coil spring movement on rear axle assembly spring seats.

#### CORRECTION:

------------ Install rear spring lower insulators, P/N 10004110 (2 required/vehicle) at the spring to axle assembly spring seat interface following applicable Service Manual procedures.

Part is currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation Number: E5057 Labor Time: 0.6 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.