INTERMITTENT OPERATION OF DECK LID OR BACK GLASS WITH REMOTE. Buick Coachbuilder 1992

For 1990-2009 cars

# INTERMITTENT OPERATION OF DECK LID OR BACK GLASS WITH REMOTE

#### SUBJECT: INTERMITTENT OPERATION OF DECK LID OR BACK GLASS WITH REMOTE KEYLESS ENTRY (INSTALL NEW RECEIVER)

#### VEHICLES AFFECTED: 1992 BUICK ROADMASTER

#### CONDITION:

---------- The deck lid or the rear back window glass may operate intermittently on the 1992 B-car, in vehicles with the Remote Keyless Entry (RKE) Option (RPO AU0).

#### CORRECTION:

----------- A new RKE receiver, P/N 10220991, was released for production effective with VIN breakpoints NR463050 on sedans, and NW408644 on wagons.

Replace the receiver, as shown in Section 9K of the Service Manual.

For vehicles repaired under warranty use:

Labor Operation: R4480 Labor Time: 0.8 Hour. Sedan 0.9 Hour. Wagon

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.