Transmission Control Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the transmission control lever boot. Refer to CELL LINK.
2. Remove the front floor console. Refer to Front Floor Console Replacement.

1

Transmission Control Fastener (Qty: 4)

Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

• | Remove the clips on the wiring harness and disconnect the shift control electrical connector.

• | Disconnect the shift control cable. Refer to Range Selector Lever Cable Adjustment.

Tighten
9 N·m (80 lb in)

2 | Transmission Control