Exhaust Temperature Sensor Replacement - Position 2. Chevrolet Cruze (GME) 2010

For 1990-2009 cars

### Removal Procedure

Warning: Refer to Exhaust Service Warning in the Preface section.

Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

1. Remove the exhaust flex pipe. Refer to Exhaust Flexible Pipe Replacement.
2. Disconnect the exhaust temperature sensor wiring harness plug (2).
3. Unclip the exhaust temperature sensor wiring harness plug (3) from the particulate filter bracket (1).
4. Remove the exhaust temperature sensor - position 2 (4).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the exhaust temperature sensor - position 2 (4) and tighten to 45 N·m (34 lb ft).
2. Clip in the exhaust temperature sensor wiring harness plug (3) to the particulate filter bracket (1).
3. Connect the the exhaust temperature sensor wiring harness plug (2).
4. Install the the exhaust flex pipe. Refer to Exhaust Flexible Pipe Replacement.