Low and Reverse and 1-2-3-4 Clutch Housing Assemble. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Table 1: | 1-2-3-4 Clutch Piston Installation
Table 2: | Low and Reverse Clutch Piston Installation

### 1-2-3-4 Clutch Piston Installation

Callout | Component Name
--- | ---

1

1-2-3-4 Clutch Piston

Tip
DT-47798 seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47798 seal protector to ease the installation of the piston.

#### Special Tool

DT-47798 Seal Protector

For equivalent regional tools, refer to Special Tools.

2 | 1-2-3-4 Clutch Spring

3

1-2-3-4 Clutch Spring Retainer

Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals.

Tip

1. Place the retainer onto DT-47799-1 which is part of DT-47799 spring compressor . Compressing the spring using DT-47799-2 which is part of DT-47799 spring compressor , will install the retainer into the retainer groove.
2. Apply shop air to the clutch fluid feed hole in the clutch housing to verify proper piston operation.

#### Special Tool

DT-47799 Clutch Piston Spring Compressor

For equivalent regional tools, refer to Special Tools.

### Low and Reverse Clutch Piston Installation

Callout | Component Name
--- | ---

1

Low and Reverse Clutch Piston

Tip
DT-47807 seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47807 seal protector to ease the installation of the piston.

#### Special Tool

DT-47807 Clutch Piston Seal Protector

For equivalent regional tools, refer to Special Tools.

2 | Low and Reverse Clutch Spring

3

Low and Reverse Clutch Spring Retainer

Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals.

Tip

1. Place the retainer onto DT-47794-1 which is part of DT-47794 spring compressor . Compressing the spring using DT-47794-2 which is part of DT-47794 spring compressor , will install the retainer into the retainer groove.
2. Apply shop air to the clutch fluid feed hole in the clutch housing to verify proper piston operation.

#### Special Tool

DT-47794 Spring Compressor

For equivalent regional tools, refer to Special Tools.