Range Selector Lever Cable Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the range selector lever cable from the transmission control. Refer to Transmission Control Replacement.

1

Range Selector Lever Cable

#### Procedure

1. Remove the range selector lever cable seal from the bulkhead.
2. Remove the range selector lever cable from the clip.
3. Remove the range selector lever cable from the lever.
4. Adjust the range selector lever cable. Refer to Range Selector Lever Cable Adjustment.