W/S WASHER BUTTON DEFORMS IN HIGH AMBIENT TEMPERATURE. Geo Metro 1990

For 1990-2009 cars

# W/S WASHER BUTTON DEFORMS IN HIGH AMBIENT TEMPERATURE

#### Subject: WINDSHIELD WASHER BUTTON DEFORMS IN HIGH AMBIENT TEMPERATURE

#### Model and Year: 1990 GEO METRO

#### TO: ALL CHEVROLET DEALERS

Some 1990 GEO Metros may experience a deformation of the windshield washer button (located on the upper right hand horizontal surface of the instrument panel) during hot ambient temperatures.

Should this occur, it is no longer necessary to replace the entire switch assembly. The plastic button by itself may now be ordered by using P/N 96065308.

The old button can be removed by grasping it by the fingers and pulling straight up (it's retained by a press fit). The new part may then be pressed in its place.

Parts are currently available from GMSPO.

Labor Operation Number: T1669

Labor Time: .2 Hours

Failure Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.