SMU - SECTION 6A1 & 6A2 - REVISED SPECIFICATIONS. Geo Metro 1996

For 1990-2009 cars

# SMU - SECTION 6A1 & 6A2 - REVISED SPECIFICATIONS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 6A1 AND 6A2 - REVISED SPECIFICATIONS

#### MODELS: 1996 GEO METRO WITH 1.0L AND 1.3L ENGINES (VINS 6, 9 - RPOS LP2, L72)

THIS BULLETIN IS BEING ISSUED TO REPLACE THE INFORMATION FOUND UNDER "SPECIFICATIONS" ON PAGES 6A1-55 AND 6A2-54 OF THE 1996 SERVICE MANUAL (GMP/96-M-1). THE SPECIFICATIONS FOUND WITHIN SECTIONS 6A1 AND 6A2 SHOULD ALSO BE UPDATED WITH THESE REVISED SPECIFICATIONS.

6A1 - 1.0L L3 (VIN 6 - RPO LP2) ===============================

FASTENER TIGHTENING SPECIFICATIONS

FLYWHEEL RETAINING BOLTS 78 N.M (56 LB FT)

HEAT SHIELD BOLTS 6 N.M (53 LB IN)

6A2 - 1.3L L4 (VIN 9 - RPO L72) ===============================

FASTENER TIGHTENING SPECIFICATIONS

CRANKSHAFT TIMING PULLEY BOLTS 16 N.M (12 LB FT)

CRANKSHAFT TIMING SPROCKET BOLT 130 N.M (96 LB FT)

FRONT PIPE/THREE WAY CATALYTIC CONVERTER ASSEMBLY-TO-EXHAUST MANIFOLD BOLTS 50 N.M (37 LB FT)

ROCKER ARM SHAFT SCREWS 25 N.M (18 LB FT)

TIMING BELT COVER NUT AND BOLTS 16 N.M (12 LB FT)

#### ENGINE SPECIFICATIONS:

=====================

#### CAMSHAFT:

CAMSHAFT TIMING SPROCKET BOLTS 60 N.M (43 LB FT)

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.