Speedometer Drive Gear Replacement. Geo Metro 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the gearshift control lever from the gearshift lever case. Refer to Gearshift Control Lever Replacement .
2. Remove the following items from the main shaft:

• | The speedometer drive gear retaining ring (2)

• | The speedometer drive gear (1)

3. Inspect the speedometer drive gear for excessive wear or damage. Replace as necessary.

### Installation Procedure

1. Install the speedometer drive gear (1) into the main shaft; secure with the speedometer drive gear retaining ring (2).
2. Install the gearshift control lever into the gearshift lever case. Refer to Gearshift Control Lever Replacement .