SERVICE MANUAL UPDATE SEC. 6A ENGINE MECHANICAL REVISED. Geo Metro 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6A ENGINE MECHANICAL REVISED

#### Subject: UNDERSIZED BEARING ART REPLACEMENT

#### Model and Year: 1 991 G EO M ETRO

Figure 1 in this bulletin replaces the chart in Figure 138 on page 6A1-42 of the 1991 GEO Metro Service Manual (ST370-91).

Refer to the table in Figure 1 for determining correct undersized bearing clearance.

#### MEASURED JOURNAL DIAMETER

| | 44.744-44.750 mm |44.738-44.744 mm |44.732-44.738 mm | | (1.7616-1.7618") |(1.7614-1.7616") |(1.7612-1.7614") | | | | LETTERS STAMPED |A| GREEN AND RED | BLACK AND RED | RED ONLY ON MATING SURFACE | | | | OF CYLINDER BLOCK |B| BLACK AND RED | RED ONLY | YELLOW AND RED | | | | |C| RED ONLY | YELLOW AND RED | BLUE AND RED | | | |

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.