SMU - SECTION 3A - REVISED SPECS. FOR WHEEL ALIGNMENT. Geo Metro 1996

For 1990-2009 cars

# SMU - SECTION 3A - REVISED SPECS. FOR WHEEL ALIGNMENT

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3A - REVISED SPECIFICATIONS FOR WHEEL ALIGNMENT

#### MODELS: 1995-96 GEO METRO

THIS BULLETIN IS BEING ISSUED TO REVISE THE INFORMATION FOUND UNDER "SPECIFICATIONS" IN SECTION 3A OF THE SERVICE MANUAL.

PLEASE UPDATE THE SERVICE MANUAL WITH THE FOLLOWING:

#### TOTAL TOE:

FRONT - 0 DEG. TO 0.32 DEG. REAR - 0.3 DEG. TO 0.6 DEG.

#### CAMBER:

FRONT - -0.5 DEG. TO 1.5 DEG. REAR -1 DEG. TO 1 DEG.

#### CASTER:

FRONT - 1 DEG. TO 5 DEG.

#### TURNING ANGLE:

INSIDE - 38 DEG. OUTSIDE - 32 DEG.

SIDE SLIP LIMIT:

FRONT - LESS THAN 3 MM/M (0.118"/1') REAR - 1 TO 5MM/M (0.039-0.197"/1')

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.