HEADLINER HAS FISHY ODOR (REPLACE HEADLINER). Buick Coachbuilder 1992

For 1990-2009 cars

# HEADLINER HAS FISHY ODOR (REPLACE HEADLINER)

#### SUBJECT: HEADLINER HAS FISHY ODOR (REPLACE HEADLINER)

#### VEHICLES AFFECTED: 1992 "B" MODEL SEDANS

THIS BULLETIN IS BEING REVISED TO CHANGE PART NUMBER FOR COLOUR SAPPHIRE.

#### APPLICATION:

----------- 1992 "B" Car Buick Roadmaster Sedans

#### CONDITION:

--------- Some owners of 1992 Buick Roadmaster Sedans may comment of a fishy odor coming from the headliner.

#### CORRECTION:

---------- Replace headliner following the procedures in the 1992 Service Manual, Section 10-9-1, using the part numbers listed below:

12521938 - Lt. Camel

12521939 - Dk. Red Maple

12521940 - Med. Dk. Gray

10226882 - Med. Gray

12521984 - Sapphire

Old stock has been removed from GMSPO,

#### WARRANTY INFORMATION:

For vehicles repaired under warranty use:

Labour Operation: C-3128

Labour Time: 0.8 Hr.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.